These depth grids are to accompany the USGS Stream Gage 15266300, which is NWSLID SXRA2.

Datum: Zero Gage datum is 40.4 ft (NAVD88)

|  |  |
| --- | --- |
| **Water Surface Elevation, feet, NAVD88** | **Gage Height (ft)** |
| 49.4 | 9 |
| 50.4 | 10 |
| 51.4 | 11 |
| 51.9 | 11.5 |
| 52.4 | 12 |
| 53.4 | 13 |
| 54.4 | 14 |
| 55.4 | 15 |
| 56.4 | 16 |
| 57.4 | 17 |

Partner attributions:

* Maps developed in cooperation with the Kenai Peninsula Borough.  [Link](http://www.kpb.us)
* Maps developed in cooperation with the Alaska Silver Jackets.  [Link](http://silverjackets.nfrmp.us/state-teams/alaska)